fifo wf^{11,40}

∀es:ES, C, T :Type, S:(C→C→E→ P), R:(C→E→ P), code:(j,i:C→e:{x:E| S(j,i,x)} →state@loc(e)→T ), decode:(i:C→e:{x:E| R(i,x)} →state@loc(e)→T ). forclients C sends FIFO

from j to i via (S[j,i],code) receives at i via (R[i],decode) ∈ P

http://www.nuprl.org/FDLcontent/p0 963683 /p31 683021 {fifo wf}.html